***Lamartine Fires & Fireplaces***

***How to use and light your B&G Infire***

1. **Clean out fire thoroughly and wipe the glass clean.**
2. **On the air control set the black knob to 9.**
3. **Turn the fan onto ½ speed.**
4. **Place your logs inside the unit in a scattered arrangement with firelighters lighting underneath.**
5. **Close over the door but do not lock it, leave it ajar while the fire is taking off for roughly 2 minutes.**
6. **After approximately 2 minutes close and lock the door. The fire will now burn for approximately 45 minutes to 1 hour on the setting 9, in this period the logs will burn down to a hot bed of ash and establish nice heat.**
7. **After the first 45 minutes to 1 hour you will now have to re-load the fire. Open the door put in more logs and now also lower the air control from 9 to roughly 4 or 5 never any lower, this is a nice setting and will make the logs last a lot longer while still producing a nice heat level. We still have the fan running at the high speed level you can now lower this if you wish, but it must always be on while the fire is burning.**
8. **When you are going to bed turn off the fan and let the fire die out.**

**NB- PLEASE USE KILN DRIED LOGS IF YOU WISH TO HAVE THE BEST BURN AND BEST HEAT IT IS ALSO VERY IMPORTANT FOR YOUR CHIMNEY AND FIRE.**

**PLEASE ALSO ENSURE YOU GET YOUR APPLIANCE SERVICED ANNUALLY TO MAINTAIN ITS GOOD WORKING AND WARRANTY**

**LAMARTINE SERVICE DEPARTMENT -01-4274610**