***Lamartine Fires & Fireplaces***

***How to use and light your Wanders Marvic Appliance***

1. **Clean out your fire and wipe the glass clean, the fire can be cleaned by lifting out the top grate inside the base of the fire and empty your ash pan also.**
2. **On the unit pull out the lever on the left hand side at hearth level and push in the lever on the right, at hearth also.**
3. **Place your logs into the fire in a scattered arrangement with the firelighters lighting underneath, once done close over the door but do not lock it ,leave it ajar for roughly 2 minutes ,this will help the fire establish and heat the glass on the inside.**
4. **After the 2 minutes or so close and lock the door, the fire will now be lit.**
5. **When these logs have burned down to a hot bed of ash you can reload the fire and now you can adjust the burning of the fire by pulling out the right hand side lever and controlling the burn by gently pushing in the left hand lever to your desired setting.**

**NB- PLEASE USE KILN DRIED LOGS IF YOU WISH TO HAVE THE BEST BURN AND BEST HEAT IT IS ALSO VERY IMPORTANT FOR YOUR CHIMNEY AND FIRE.**

**PLEASE ALSO GET YOUR APPLIANCE SERVICED ANNUALLY TO MAINTAIN ITS GOOD WORKING AND WARRANTY**

**LAMARTINE SERVICE DEPARTMENT -01-4274610**