***Lamartine Fires & Fireplaces***

***How to use and light your Wanders SQ Woodburner***

1. **Clean out fire thoroughly and wipe the glass clean.**
2. **Pull out your air control full out.**
3. **Place your logs inside the unit in a scattered arrangement with the firelighters lighting underneath on top of the ash.**
4. **Close over the door but do not lock it, leave it ajar while the fire is taking off for approximately 1-2 minutes.**
5. **After the 1-2 min’s close and lock the door. The fire will now burn for roughly 45 minutes to 1 hour with the lever out fully, in this period the logs will burn down to a hot bed of ash and establish nice heat .**
6. **After the first 45 min’s to 1 hour you will now have to reload the fire. Open the doors put in more logs and now also push the air control handle in half way. By doing this you will now get longer out of your logs and a nice heat level.**
7. **Top up the fire every so often to keep it alight.**

**NB- PLEASE USE KILN DRIED LOGS IF YOU WISH TO HAVE THE BEST BURN AND BEST HEAT IT IS ALSO VERY IMPORTANT FOR YOUR CHIMNEY AND FIRE.**

**PLEASE ALSO GET YOUR APPLIANCE SERVICED ANNUALLY TO MAINTAIN ITS GOOD WORKING AND WARRANTY**

**LAMARTINE SERVICE DEPARTMENT -01-4274610**